PROGRAM

INCLUDE software serial

INITIALIZE softwareserial GPS(TX pin, RX pin)

ASSIGN data to space

FUNCTION setup

ASSIGN serial begin to 115200 speed

ASSIGN GPS begin to 9600 speed

END FUNCTION

FUNCTION loop

IF GPS() available

ASSIGN data to read GPS

PRINT serial(data)

END IF

END FUNCTION

END PROGRAM